

                                  TFM v1.0.1  -  HELP FILE  (02/19/2007)



CONTENTS OF FILE:


    A.) General Info
    B.) Basic Parameters
    C.) Advanced Parameters
    D.) File Input/Output Parameters
    E.) Debug/Display Parameters
    F.) Overrides Info
    G.) Change List
    H.) To Do List



A.)  GENERAL INFO:


     * Currently TFM only supports YV12 and YUY2 colorspaces!

      TFM is a field matching filter that recovers the original progressive frames from a
   telecined stream.  It does not decimate the resulting duplicate frames though, so to
   achieve an ivtc you must follow TFM with a decimation filter such as TDecimate(), which
   is also included in the TIVTC dll.


   syntax=>

       TFM(int order, int field, int mode, int PP. string ovr, string input, string output,
            string outputC, bool debug, bool display, int slow, bool mChroma, int cNum,
            int cthresh, int MI, bool chroma, int blockx, int blocky, int y0, int y1,
            int mthresh, PClip clip2, string d2v, int ovrDefault, int flags, double scthresh,
            int micout, int micmatching, string trimIn, int hint, int metric, bool batch,
            bool ubsco, bool mmsco, int opt)


      While TFM does have quite a few parameters, I have tried to categorize the settings so
   they are easier to manage.  Really there are only 3 parameters most users should be
   concerned about knowing or ever setting.  They are "order", "mode", and "PP" and are
   described under the "BASIC PARAMETERS" sections.  The other settings are described under
   the other various sections which should be pretty easy to figure out from the names.



B.)  BASIC PARAMETERS:


   These are the only three parameters most users should be concerned with or worry about
   setting.  They control the basic operation of the filter.


     order - 

        Sets the field order of the clip. The field order must be correctly set for
        accurate field matching to occur. Possible values:

           -1 = auto (use avisynth's internal parity value)
            0 = bottom field first (bff)
            1 = top field first (tff)

        Default:  -1  (int)


     mode - 

        Sets the matching mode or strategy to use.  Plain 2-way matching (option 0) is the
        safest of all the options in the sense that it wont risk creating jerkiness due to
        duplicate frames when possible, but if there are bad edits or blended fields it will
        end up outputting combed frames when a good match might actually exist.  3-way matching
        + trying the 4th/5th matches if all 3 of the original matches are detected as combed
        (option 5) is the most risky in terms of creating jerkiness, but will almost always
        find a good frame if there is one.  The other settings (options 1, 2, 3, 4, and 6) are all
        somewhere in between options 0 and 5 in terms of risking jerkiness and creating
        duplicate frames vs. finding good matches in sections with bad edits, orphaned fields,
        blended fields, etc...

        Mode 7 is is not one of the normal modes and is specifically for material with blended
        fields that follows a specific pattern.  Mode 7 requires linear access to work correctly
        because what match/field are used depends on previous match decisions.

        Possible settings are:

            0 = 2-way match                                                          (p/c)
            1 = 2-way match + 3rd match on combed                                    (p/c + n)
            2 = 2-way match + 3rd match (same order) on combed                       (p/c + u)
            3 = 2-way match + 3rd match on combed + 4th/5th matches if still combed  (p/c + n + u/b)
            4 = 3-way match                                                          (p/c/n)
            5 = 3-way match + 4th/5th matches on combed                              (p/c/n + u/b)
            6 = mode 2 + extras if combed                                            (p/c + u + n + b)
            7 = mode 0 + field switching based on previous matches

        The () at the end indicate the matches that would be used for that mode assuming order = 1
        and field = 1.

           * In terms of speed option 0 is by far the fastest and 5 is the slowest.

        Default:  1  (int)


     PP -

        Sets the post-processing mode.  This controls how TFM should handle (or not handle)
        any combed frames that come out of the field matching process.  Possible options
        are:

            0 - nothing (don't even look for combed frames)
            1 - find/hint combed frames but don't deinterlace
            2 - dumb blend deinterlacing
            3 - dumb cubic interpolation deinterlacing
            4 - dumb modified-ela deinterlacing
            5 - motion-adaptive blend deinterlacing
            6 - motion-adaptive cubic interpolation deinterlacing
            7 - motion-adaptive modified-ela deinterlacing

           * You can also use the "clip2" parameter to specify an externally deinterlaced clip
             from which TFM will take frames instead of doing the deinterlacing itself.  See
             the clip2 parameter description for more info and to see how the PP settings effect
             operation with clip2.

           * You can manually control what frames should be marked as combed as well as the
             PP option through an overrides file (see the ovr parameter description)

        Default:  6  (int)



C.)  ADVANCED PARAMETERS:


   These parameters give finer control over the matching operation, combed frame detection,
   and deinterlacing of combed frames.  While correctly tweaking these values can increase
   matching accuracy they can also make things worse.


     field - 

         Sets the field to match from.  It is recommended to set this to the same value
         as order unless you experience matching failures with that setting.  In certain
         circumstances changing the field that is used to match from can have a large impact
         on matching performance. Possible values are:

           -1 = auto (TFM will set field to the same value as the order parameter)
            0 = bottom field
            1 = top field

         Default:  -1  (int)


     slow -

         Sets which field matching fuction is used.  Possible settings:

            0 - normal   (should have the worst accuracy)
            1 - slower
            2 - slowest  (should have the best accuracy)

         This is basically a quality vs. speed option (the slower the function the more
         accurate it should be).  Prior to v0.9.9.1 of tfm this was a boolean value, true
         from previous versions corresponds to a current value of 1 and false corresponds
         to a current value of 0.

         Default:  1  (int)


     mChroma -

         Sets whether or not chroma is included during the match comparisons.  In most
         cases it is recommended to leave this enabled.  Only if your clip has bad chroma
         problems such as heavy rainbowing or other artifacts should you set this to false.
         Setting this to false could also be used to speed things up at the cost of some 
         accuracy.

            true = chroma is included
            false = chroma is not included

         Default:  true  (bool)


     y0/y1 -

         These define an exclusion band which excludes the lines between y0 and y1 from
         being included in the field matching decision.  An exclusion band can be used
         to ignore subtitles, a logo, or other things that may interfer with the matching.
         y0 sets the starting scan line and y1 sets the ending line, all lines in between
         y0 and y1 (including y0 and y1) will be ignored.  Set y0 equal to y1 to disable.

         Default:  y0 - 0  (int)
                   y1 - 0  (int)


     scthresh -

         Sets the scenechange threshold as a percentage of maximum change on the luma plane.
         Good values are in the 8.0 to 14.0 range.  Scenechange detection is used by the
         following parameters:  ubsco, mmsco, and flags (only flags=5).  The range for
         scthresh is [0.0, 100.0].

         Default:  12.0  (double)


     ubsco -

         Allow u/b matches to be used only around scenechanges.  The 'scthresh' parameter sets the
         scenechange threshold as a percentage of maximum change on the luma plane.  To disable
         this (allow u/b matches everywhere) set ubsco to false.  The ubsco setting only effects
         automatic matching, i.e. u/b matches via an overrides or input file are not changed.
         The only matching modes that ubsco is used with are 2, 3, 5, and 6 (the only ones that
         use u/b matches).

         Default:  true (bool)


     micmatching -

         When micmatching is greater than 0, tfm will take into account the mic values of matches
         when deciding what match to use as the final match.  micmatching has 5 possible settings:

           0 - disabled
           1 - mics are only used to determine if of the 5 possible matches there is one match
                  that has a significantly lower mic value than all of the other four matches.
                  With this option enabled it is possible for tfm to use any match (p/c/n/b/u)
                  regardless of the matching mode!
           2 - use mics to aid the decision within the current matching mode (only matches that
                  could be used within the current matching mode are considered)
           3 - do both option 1 and option 2
           4 - do a post field matching decision check only (this operation is included in
                  micmatching modes 1, 2, and 3, and is not subject to the mmsco parameter)

         Debug output will indicate when micmatching has led to a change in the match decision.
         Enabling micmatching will make processing slower due to needing to calculate mic values
         for matches that they normally wouldn't be calculated for.

         The "mmsco" parameter can be used to restrict the use of micmatching to scenechanges only.
         To do this, set mmsco to true... then, only frames on either side of a scenechange
         will have the possibility of being effected by micmatching.

            **** As of v0.9.10.0 of TFM, micmatching defaults to 1. That means any one of the five
            **** matches could be used regardless of the matching mode!  If you don't want this
            **** behavior then set micmatching to 0!

            **** As of v0.9.12.6 of TFM, all micmatching modes will run a check after each
            **** field matching decision to check for cases where the mic values make it
            **** obvious that the wrong match was chosen.  This part acts independently of
            **** the mmsco parameter.

         Default:  1  (int)


     mmsco -

         Allow micmatching around scenechanges only.  The 'scthresh' parameter sets the
         scenechange threshold as a percentage of maximum change on the luma plane. If set
         to true, then micmatching will be limited to scenechanges only.  If set to false,
         then micmatching will be allowed anywhere.

         Default:  true (bool)


     hint -

         Enables writing hint information into the video frames for tdecimate or tdeint to read.
         Information includes match used, combed vs. progressive, and d2v rff info. true enables
         writing, false disables.

         Default:  true (bool)


     opt -

         Controls which optimizations are used.  Possible settings:

            0 - use c routines
            1 - use mmx routines
            2 - use isse routines
            3 - use sse2 routines
            4 - auto detect

         Default:  4  (int)


   The rest of the "advanced parameters" control combed frame detection and deinterlacing,
   and are only used if mode is set to 1, 2, or 4 or PP (post-processing) is set to 1 or greater!


     cthresh -

         This is the area combing threshold used for combed frame detection.  It is like
         dthresh or dthreshold in telecide() and fielddeinterlace().  This essentially
         controls how "strong" or "visible" combing must be to be detected.  Larger values
         mean combing must be more visible and smaller values mean combing can be less
         visible or strong and still be detected.  Valid settings are from -1 (every pixel
         will be detected as combed) to 255 (no pixel will be detected as combed).  This
         is bascially a pixel difference value.  A good range is between 8 to 12.

         Default:  9  (int)


     chroma -

         Sets whether or not chroma is considered in the combed frame decision.  Only
         disable this if your source has chroma problems (rainbowing, etc...) that are
         causing problems for the combed frame detection with chroma enabled.  Actually,
         using chroma=false is usually more reliable, except for the case that there
         is chroma only combing in the source.

            true = chroma is included
            false = chroma is not included

         Default:  false  (bool)


     blockx -

         Sets the x-axis size of the window used during combed frame detection.  This has
         to do with the size of the area in which MI number of pixels are required to be
         detected as combed for a frame to be declared combed.  See the MI parameter
         description for more info.  Possible values are any number that is a power of
         2 starting at 4 and going to 2048 (i.e. 4, 8, 16, 32, ... 2048).

         Default:  16  (int)


     blocky -

         Sets the y-axis size of the window used during combed frame detection.  This has
         to do with the size of the area in which MI number of pixels are required to be
         detected as combed for a frame to be declared combed.  See the MI parameter
         description for more info.  Possible values are any number that is a power of
         2 starting at 4 and going to 2048 (i.e. 4, 8, 16, 32, ... 2048).

         Default:  16  (int)


     MI -

         The # of combed pixels inside any of the blocky by blockx size blocks on the frame
         for the frame to be detected as combed. While cthresh controls how "visible" the
         combing must be, this setting controls "how much" combing there must be in any localized
         area (a window defined by the blockx and blocky settings) on the frame.  Min setting = 0,
         max setting = blocky x blockx (at which point no frames will ever be detected as combed).

         Default:  80  (int)


     metric -

         Sets which spatial combing metric is used to detect combed pixels.  Possible
         options:

              Assume 5 neighboring pixels (a,b,c,d,e) positioned vertically.

                    a
                    b
                    c
                    d
                    e

            0:  d1 = c - b;
                d2 = c - d;
                if ((d1 > cthresh && d2 > cthresh) || (d1 < -cthresh && d2 < -cthresh))
                {
                   if (abs(a+4*c+e-3*(b+d)) > cthresh*6) it's combed;
                }

            1:  val = (b - c) * (d - c);
                if (val > cthresh*cthresh) it's combed;

         Metric 0 is what tfm used previous to v0.9.12.0.  Metric 1 is the combing metric used
         in Donald Graft's FieldDeinterlace()/IsCombed() funtions in decomb.dll.

         Default:  0  (int)


     mthresh -

         Sets the motion (pixel difference) threshold for deinterlacing when using motion
         adaptation (PP > 4).  As said, it is simply a pixel difference threshold between
         frames... if under mthresh then a pixel is considered static, if over mthresh it is
         considered moving.

         Default:  5  (int)


     clip2 -

         When using PP > 1 this parameter may be used to specify a clip to take deinterlaced
         frames from instead of using one of TFM's inbuilt deinterlacing methods.  If PP < 5
         then frames will be taken as is from clip2, if PP >= 5 (i.e. using motion adaptation)
         then TFM will build the mask as usual and only pixels in moving areas will be taken
         from the frames in clip2. Don't specify anything for clip2 to use TFM's internal
         deinterlacing.  For an example of using clip2 see the clip2_sample_avs.avs file.

         Default:  NULL  (PClip)



D.)  FILE INPUT/OUTPUT PARAMETERS:


   These settings deal with overrides file usage and output/input file options.


     d2v -

        This option is intended to be used if you are using an mpeg2source() with a d2v file.
        It sets the name and path to a d2v file, which TFM will analyze to see if there are any
        illegal field order changes and optionally set the order parameter using the field
        order of the d2v file.  If the d2v file is found to have illegal field order transitions,
        TFM will create a fixed d2v file with the string "-FIXED" attached to the end of the file
        name.  The new file will be located in the same directory as the original.  You can then
        use this fixed d2v file for processing.  If the order parameter is set to "-1" then TFM
        will detect the field order from the d2v file and set the order parameter to match. Depending
        on the value of the "flags" parameter, TFM will also use the d2v info for field matching
        and will pass info from the d2v on to tdecimate to help aid duplicate detection and hybrid
        detection.

            *NOTE:  This option currently supports all d2v formats that I am aware of... which
                    include:  dvd2avi 1.76, 1.77.3 and its variants, all dvd2avidg versions, and
                    all dgindex versions.

            example =>  TFM(d2v="myd2v.d2v")

        Default:  ""  (String)


     flags -

        Controls how much of the info from the d2v file is used when the "d2v" parameter is set.
        Possible options:

           0 - Check the d2v file for illegal transitions and set the order parameter if it
                  is not already manually set.  Also, pass on rff flag duplicate info to
                  tdecimate.
           1 - Same as 0, plus use the trf flags for field matching in film sections (sections
                  where the trf flags follow the 012301... pattern)
           2 - Same as 1, but use the trf flags for field matching in all areas (doesn't have
                   to be in 0123 pattern)  (very much not recommended!)
           3 - Same as 0, but don't pass on any info to tdecimate (i.e. only set order and check
                   for illegal transitions)
           4 - Same as 1, but d2v matches are checked for being combed.  If a d2v match is detected
                   as combed then tfm uses its own matching routine for that frame.
           5 - Same as 4, but d2v matches are only checked for being combed around scenechanges.

           VERY IMPORTANT (MUST READ):  For options 0, 1, 2, 4, and 5 to work correctly, tfm/tdecimate
                                        must either immediately follow the mpeg2source() command or
                                        any filters inbetween them must not modify the order or number
                                        of fields in the stream in any way. Or use a trimIn file to
                                        tell TFM what frames have been discarded.

        Default:  4  (int)


     trimIn -

         Allows using the d2v="" option with flags = 0, 1, 2, 4, and 5 while having trim() statements
         before TFM.  To use a trimIn file simply create a new file and set trimIn="PATH\file.txt". The
         file should list the ranges of frames that were NOT kept... for example, let's say the original
         file has 30000 frames but you remove the first 100 by using trim(100,0) before tfm.  Then in
         the trimIn file you would have the following entry:

              0,99

         So you simply specify the ranges of frames that are no longer present.  You can have as many
         ranges as you want (for example if you want to cut out multiple sections) and they can be
         specified in any order.  To specify a single frame, such as 10, just use:

              10,10

         Default:  ""  (String)


     ovr -

        Sets the name and path to an overrides file.  An overrides file allows for manual control
        over what matches are used for specific frames and ranges of frames, for changing the
        values of the field, mode, order, mthresh, PP, and MI parameters for specific frames or ranges
        of frames, and for specifiying whether or not a frame should be consider combed or not
        combed.  For more information on using an overrides file see the OVERRIDES section at the
        bottom of this file.  You can specify an ovr file and an input file at the same time.
        Matches and combed frames given in the overrides file will take precedence over those in
        the input file.

            example =>   TFM(ovr="myOvrFile.txt")

            * NOTE:  The ovr option CANNOT read output files (files made via the output option).
                     To read output files use the input parameter.

        Default:  ""  (String)


     ovrDefault -

        This is an extra option that allows you to change the default "combed" action taken when
        using an ovr file.  By default, if you don't specify a frame as combed '+' or not combed '-'
        in an overrides file then TFM just processes it as usual.  However, with the ovrDefault
        option, you can make TFM mark all frames you don't explicitly specify as either combed
        or not combed.  Basically, its an easy way to only deinterlace a few specific frames in
        a file and make sure no other frames are touched or vice versa.  If no ovr file is
        used then this setting does nothing.  Possible settings:

              0 - normal processing
              1 - mark all frames not specified in ovr file as clean (not combed)
              2 - mark all frames not specified in ovr file as combed

        Default:  0  (int)


     output -

        Sets the name and path for an output file.  TFM will create the specified file and
        output all the matches and combed frame decisions used to it.  Each line will contain
        a frame number, the match used, and the combed frame decision used.  This file
        can then be used later for input via the input parameter (so that the matches wont
        have to be recalculated).  The output file will also contain the mic value for the
        match used on each frame and the mic values for other matches if micout > 0.

        Default:  ""  (String)


     input -

        This option is meant to be used with the output option.  If you have used the output
        option on a previous pass then to reuse that info set the input parameter to the name
        and path of the output file.  You can specify both an input file and an ovr file at
        the same time.  In such a case, matches in the overrides file will take precedence.
        The input option CANNOT read ovr files!!!  To read an ovr file you must use the ovr
        parameter!

        Default:  ""  (String)


     outputC -

        This option can be used to help identify 30fps progressive video sections by outputting
        the ranges over which at least "cNum" of consecutive matches were matched as 'c'.  This
        option isn't fool proof, as slow or static film scenes can also generate long series of
        consecutive 'c' matches.

        Default:  ""  (String)


     cNum -

         Number of consecutive 'c' matches required to output a range when using the outputC
         option.

         Default:  15  (int)


     batch -

         Disables crc checking of the current video with the crc in the input file.

         Default:  false  (bool)



E.)  DEBUG/DISPLAY PARAMETERS:


   These settings control whether debug information is output or if display information
   is drawn on the frames.  These options can be useful when using overrides or when trying
   to assess matching failures.


     debug -

         If set to true, information will be output via OutputDebugString() during
         processing concerning TFM's internal operations.  Info includes: match
         comparision statistics, match used, what matches were detected as combed
         (if in modes 1, 2, or 4 or PP > 0), and the values of field, mode, order, and MIC.
         To view this information you can use a utility called "DebugView" available for
         free from:  

                http://www.sysinternals.com/ntw2k/freeware/debugview.shtml

            true = enables output
            false = disables output

         Default:  false  (bool)


     micout -

         Only used with debug=true, display=true, or output.  It forces tfm to calculate
         the MIC values for certain matches and output them with the debug and/or display
         info or include them in the output file.  Possible settings:

            0 - don't force calculation
            1 - calculate p/c/n
            2 - calculate p/c/n/b/u

         Default:  0 (int)


     display -

         If set to true, information will be drawn on the video frames themselves
         in the upper left hand corner.  This info is not as detailed as the debug
         output and only includes the current frame number, the values of mode,
         field, order, and MIC the match that was used for the current frame, and whether
         or not the output frame was combed if PP > 0.  This option can be useful
         when using overrides and you need to see what match is currently being used.
         If you need more detailed information, such as the match statistic numbers
         or to see if specific matches were detected as combed then you'll need to
         use debug output.  As of v0.9.1 display will also indicate if the final
         output frame is combed and whether or not it was deinterlaced if PP > 0.
         If PP = 1 and display is enabled, then TFM will draw a white box around the
         area of the frame that triggered its detection as combed when a frame is
         found to be combed through its internal detection (this wont be done if a
         frame is forced to be combed through overrides).

            true = enables
            false = disables

         Default:  false  (bool)



F.)  OVERRIDES:


  This section gives an explanation of how to specify overrides, what each type of
  match means, and the list of possible overrides.


  BACKGROUND AND OVERVIEW:

     Before we get started there is one thing that needs to be understood, and that is
     what in the hell the p, c, n, b, and u letters mean and where they come from.
     Well, actually, before that we need to know what field matching actually does.  I
     am going to assume that the reader knows what is meant by saying a stream is
     telecined though.  Now, consider we have the following telecined stream with the
     bottom and top fields given as follows (1t and 1b are both assumed to come from
     the same progressive frame, as are 2t and 2b, etc...):


              1t  2t  2t  3t  4t  <= original stream
              1b  2b  3b  4b  4b


     Now what TFM does, as does any field matcher, is matches the fields so that only
     progressive frames remain; however, it does not decimate duplicates.  So, the above
     input stream gets transformed into one of the two following scenarios (which one
     depends on the field we are matching from, i.e. the value of the "field" parameter):


         field = 0  (matching from bottom)

              1t  2t  3t  4t  4t   <= output stream
              1b  2b  3b  4b  4b

               c   c   n   n   c   <= matches used


         field = 1  (matching from top)

              1t  2t  2t  3t  4t   <= output stream
              1b  2b  2b  3b  4b

               c   c   p   p   c   <= matches used


      From this example, you can see why the field setting can have an impact on the
      matching performance...  Anyways, now that we have an idea of what is happening
      we can move on to what p, c, n, b, and u mean.  Basically, these letters just stand
      for what match is used.  As you can see from the above example, c means that the
      field from the current frame and of the opposite parity to that of the field being
      matched from is used, p means the field of the opposite parity to the field we are
      matching from and from the previous frame is used, and n means the field of the
      opposite parity and from the next frame is used.  These three matches, p, c, and n
      are the most common or the usual matches.  In the mode parameter description these
      are the three matches that make up the 2-way and 3-way matching.  The other matches:
      u and b  are slightly different in that they don't use the field that is being matched
      from.  In the mode parameter description these two matches are the 4th/5th matches.
      A visual explanation of all of this would probably explain things much better, so here
      are the visual representations of each match:


            * In the following examples it is assumed that we are currently matching
              the second frame (2t/2b).  Also, an "x" has been placed next to both the
              top field and the bottom field that will be used due to the current match.


        field = 0:


              c             p             n             b             u          <= match

              x         x                    x          x             x
           1t 2t 2t     1t 2t 2t       1t 2t 2t      1t 2t 2t      1t 2t 2t      <= stream
           1b 2b 3b     1b 2b 3b       1b 2b 3b      1b 2b 3b      1b 2b 3b
              x            x              x          x                   x

              2t           1t             2t            2t            2t         <= output frame
              2b           2b             2b            1b            3b



        field = 1:


              c             p             n             b             u          <= match

              x            x              x          x                   x
           1t 2t 2t     1t 2t 2t       1t 2t 2t      1t 2t 2t      1t 2t 2t      <= stream
           1b 2b 3b     1b 2b 3b       1b 2b 3b      1b 2b 3b      1b 2b 3b
              x         x                    x          x             x

              2t           2t             2t            1t            2t         <= output frame
              2b           1b             3b            2b            2b


      Well, that should pretty well do it. There are a couple other points though.
      One, you can see from the above examples that the matches have different meanings
      depending on the value of the "field" parameter.  That is why in all ovr files
      you can specify the field value with respect to which the matches in the file are
      made.  This is so that when you specify an n, p, etc... match in an ovr file, TFM
      knows for sure what you mean.  You don't HAVE to specify the reference field though,
      if you don't give one TFM simply assumes you mean to use the same value as the
      current internal field value.   However, it is much safer to specify the value.
      The second point stems from the first point, and is simply that if the reference
      field you use for an ovr file is different from that of the internal field value
      then the matches will be switched accordingly so everything is the same.  However,
      this means that if your using debug or display output the matches wont be the same
      as the ones in your ovr file.  So for reference here are the conversions or
      equivalencies...


             with Field = 0 ___ is the same as ___ with Field = 1 and vice versa

                             p        ==        b
                             c        ==        c
                             n        ==        u
                             b        ==        p
                             u        ==        n


  SYNTAX AND USING OVERRIDES:


      match codes:

              * See background/overview section for visual representation of matches.
                For range of frames overrides you can specify multiple match codes
                on the same line and the given pattern will be repeated over the length
                of the range.

         p = match to previous field
         c = match to current field
         n = match to next field
         b = match to previous field  (matches from opposite parity field)
         u = match to next field      (matches from opposite parity field)


      combed frame codes:

             * These can be used to manually force specific frames to be consider combed or
               clean.  You can specify patterns of combed frame codes like you can with
               match codes.

         + = force frame to be considered combed
         - = force frame to be considered not combed


      parameter codes:

             * Parameter codes, unlike match codes, also require a value to change to
               when used in overrides file.

         f = field
         o = order
         m = mode
         M = mthresh
         P = PP
         i = MI


      reference field:

         Since the match codes take on different meanings depending on the field parameter, you
         can specify a reference field for an overrides file.  All the matches given in file
         are then taken to be with respect to the given field.  If a reference field is not
         given then all matches are taken to be with reference to the filters internal field
         value.

         To specify the reference field you must put one of the following two lines as the
         VERY FIRST active line in the file:

              field = top
              field = bottom

         The first one would set the reference field to top (1) and the second would set it to
         bottom (0).  For an example see the included example ovr file included in the filter
         zip file.


      override syntax:

           single frame =>  frame_number code(s) [change_value]    [] = only required for parameter codes

           frame range =>   start_frame,end_frame code(s) [change_value]


      examples:

           0,100 pcpcbuu       will repeat the given pattern "pcpcbuu" of matches starting at
                                  frame 0 and ending at frame 100

           101 p               will use match p for frame 101

           300,400 c           will use match c for frames 300 through 400

           100,150 f -1        will set the field parameter to -1 for frames 100 through 150

           500,750 m 1         will set the mode parameter to 1 for frames 500 through 750

           871 o 1             will set the order parameter to 1 (tff) for frame 871

           3000,4231 cccpp     will repeat the cccpp pattern from frame 3000 till frame 4231

           4343 u              will use match u for frame 4343

           ;756 p              will be ignored

           #what is this?!?!   will be ignored

           70 -                will force frame 70 to be considered clean (not combed)

           60,80 +             will force frames 60 through 80 to be considered combed

           70,97 +--++         will force frames 70 to 97 to be considered combed or not combed
                                  as indicated by the pattern given

           87,100 P 2          will set the PP parameter to 2 for frames 87 through 100

           200 M -1            will set the mthresh parameter to -1 for frame 200

           10,20 i 100         will set MI to 100 for frames 10 through 20



      other things to know/remember:

           1.) Ranges are inclusive.

           2.) For parameter codes, the changed value is always set back to what it was
               originally set to after the override goes out of the specified range.
               (i.e. if you specify a field override for frame 600 to 700 after frame
               700 field is set back to its original value automatically, you don't need
               to set it back in the overrides file!  The original value is what it is
               set to on load (i.e. either the default or what you set it to in your
               avisynth script).

           3.) Frame numbers must be within range for the file.

           4.) Frame numbers for match codes must be ascending, and frame numbers for the
               same parameter codes must not overlap!!!  In other words, don't make
               multiple overrides for the same parameter over the same range of frames.

           5.) The spacing is important!  (no spaces between the comma and frame numbers,
               one space between the end frame number and the specifier, one space between
               the specifier and the value to change to if it has one). Just look at the
               examples for clarification.

           6.) Only match codes and combed frame codes can be used in pattern specifications.
               Pattern specifications can be up to 50 match codes maximum.

           7.) To comment out a line (have TFM ignore it) in an ovr file, you can
               either put a '#' symbol or ';' at the beginning of the line.

           8.) An example ovr file w/ comments is included in the filter zip file for reference.

           9.) Setting the second frame in a range to 0 means the same as setting it to the
               last frame of the clip.



G.)  CHANGE LIST:


    02/19/2007  v1.0.1

         + Support d2v file format v16
         - fixed a bug in tfmpp destroying hints
         - fixed generating ovr help info about combed frames in output files when PP=0


    01/18/2007  v1.0

         + Support d2v file format v15 and remove check for newer d2v formats


    12/21/2006  v0.9.12.8

         + Support d2v file format v14


    11/26/2006  v0.9.12.7

         - expanded file input line buffers from 80 bytes to 1024 bytes


    11/04/2006  v0.9.12.6

         + micmatching modes 1, 2, and 3 now check each match decision for cases where the
             correct match is obvious based off mic values but the field matching routine
             is unable to distinguish the correct match
         + added micmatching mode 4, does the post match decision check and nothing else


    10/22/2006  v0.9.12.5

         + preserve hints from dgdecode through tfm
         + added flags=5 option... same as 4, except that only frames around scenechanges are checked
              for being combed
         + changed 'sco' to 'scthresh' and added 'ubsco' and 'mmsco' parameters.  Using u/b matches
              only around scenechanges and using micmatching only around scenechanges are now
              controlled with separate parameters.
         - fixed incorrect d2v duplicate marking by tfm when using hints and not using linear,
              forward play
         - fixed frames with 'h' and 'l' matches not being correctly overridden by an ovr file


    10/03/2006  v0.9.12.4

         + Added batch option (disables input file crc checking)
         + Display crc values in error msg when crcs don't match


    07/26/2006  v0.9.12.3

         - fixed crash in modes 0/4 when pp=0 and micout > 0
         - fixed "possible missed combed frames" listing in ovr help information
              sometimes including frames that were marked combed via an ovr file


    05/08/2006  v0.9.12.2

         + output file generation is now effected by the micout parameter
         + if micout > 0 then calculate/output mics even when an override or d2v
               match is used
         - fixed a bug introduced in the last release in cubic deint pping (pp=3/6)
         - fixed a bug in one of the yuy2 checkcombed mmx assembly routines


    04/09/2006  v0.9.12.1

         + minor field matching improvements
         + optimized postprocessing (mmx/sse2 cubic/blend deint, mmx/sse2 motion map creation,
              mmx/sse2 clip2 copy, faster link/denoise routines)
         + added ovr help information listing to bottom of output file
         - call setcachehints for clip2 when used


    03/23/2006  v0.9.12.0

         + Added metric parameter and new spatial combing metric
         + Added hint parameter
         - throw an error if the field order of a d2v does not match the
              user specified field order
         - replace frame copy with makewritable where possible
         - fixed cthresh < 0 not working correctly


    01/24/2006  v0.9.11.4

         + slow=0 matching mode optimizations
         + mmx version of isse/sse2 check_combed routine
         + added opt parameter
         - fixed sse2 routines using psrldq


    01/19/2006  v0.9.11.3

         + assembly optimizations


    01/17/2006  v0.9.11.2

         + Support d2v format version 13
         + Write MIC values into output file
         + A few new mmx/isse optimizations
         + sse2 optimizations (only used on P4)
         - Fixed clip2 crash caused by writing to a referenced frame
         - Fixed rare crash on d2v input parsing caused by sometimes writing
             one entry past the end of an array


    12/03/2005  v0.9.11.1

         + Added mmx versions of the isse scenechange routines
         + Optimized combed frame detection routines


    11/01/2005  v0.9.11.0

         + Added trimIn parameter
         + Minor field matching improvement


    10/14/2005  v0.9.10.2

         + micmatching can now be limited to scenechanges only, via the "sco" parameter
         + slow=1/2 matching mode optimizations (~10% speed increase)
         + display output now shows when scenechanges are detected when sco > 0
         - changed sco default to 12.0


    10/12/2005  v0.9.10.1
 
         + support dgindex d2vformat v12


    09/28/2005  v0.9.10.0

         + Allow MI to be changed via overrides (same as field/mode/order/etc...)
         + Added mode 7 matching routine (specifically for material with blended fields)
         - changed default MI value to 80
         - changed default cthresh value to 9
         - changed default micmatching value to 1
         - fixed description of micmatching in help file


    09/21/2005  v0.9.9.7

         + Field matching improvements
         + micmatching changed from bool to int, added micmatching 2/3 options
         - flags parameter now defaults to 4
         - Fixed IsCombedTIVTC always resulting in an error being thrown (was
              introduced when micout was added)


    09/15/2005  v0.9.9.6

         - Fixed micmatching parameter not being initialized correctly


    09/11/2005  v0.9.9.5

         + Added flags=4 option
         - when micmatching=true only calculate the extra mics if the mic value for the would
             be final match is > 15


    09/02/2005  v0.9.9.4

         + Added micmatching parameter
         + micout now works with display output
         - stricter checking for 0123 sections with flags=1
         - fixed a few debug output format inconsistencies


    08/27/2005  v0.9.9.3

         + Added v11 d2v format support
         + Field matching improvements (improved the code that decided which metrics
               to use when picking the final match)
         + Added micout parameter


    08/14/2005  v0.9.9.2

         + Added sco parameter (u/b matches only at scenechanges)


    07/31/2005  v0.9.9.1

         + Added slowest matching fuction and changed the parameter "slow" from bool to int


    07/31/2005  v0.9.9

         + Added new match mode (mode 6)
         + Added field matching from d2v file and flags parameter to better control
              how the d2v info is used


    06/25/2005  v0.9.8.1

         + Added support for new dgindex d2v's (d2vformat v10)


    06/06/2005  v0.9.8

         + Added a new match mode (mode 2, old mode 2 is now mode 3, 3 is 4, and so on)
         + Added support for new dgindex d2v's (d2vformat v9)


    04/20/2005  v0.9.7.3

         + Debug and display options now output a value called MIC (the value that is computed
              and compared against MI to check if a frame is combed) to make tweaking
              the MI parameter easier.  The MIC value is computed during combed frame detection and
              is the single highest value computed for any one of the blockx by blocky sized blocks.
              Previously, combed frame detection exited immediately upon finding the first block
              with an MIC value greater than MI... it now scans all blocks and returns the highest.
              Thus, the white box that is drawn when display=true, PP=1, and a frame is detected
              as combed now corresponds to the block with the highest MIC value and not the first
              to be found.
         - Changed default MI value to 85 (also changed to 85 in IsCombedTIVTC)
         - Fixed the white box drawn on combed frames when PP=1 sometimes being drawn in the
              incorrect spot when mode was set to 1, 2, or 4


    03/13/2005  v0.9.7.2

         + Post-processing now only links luma->chroma on the motion map, instead of doing full
              luma->chroma, chroma->luma, and chroma->chroma linking.


    03/10/2005  v0.9.7.1

         - Fixed a crash that would occur if the d2v option was enabled and a trim() or some other
              filter that altered the number of frames was used prior to tfm()


    02/19/2005  v0.9.7

         + Added support for new dgindex project file versions 07 and 08 (dgindex v1.2) to the d2v option.
         - Fixed the d2v method of fixing illegal transitions.
         + TFM now uses the rff flags from the d2v to help tdecimate identify duplicates and 24p film.
         - Changed default MI value to 100.
         - Fixed the readme file indicating chroma=true, when it actually defaults to false


    01/08/2005  v0.9.6.3

         - Fixed SetCacheHints being called incorrectly and always defaulting to CACHE_ALL


    01/02/2005  v0.9.6.2

         - Changed the d2v method of fixing illegal transitions to one that doesn't alter
              the total # of fields in the clip or the # of fields from each of the original
              frames in the stream.
         - Changed default value for the chroma option to false
         + Some other optimizations and internal changes.


    12/22/2004  v0.9.6.1

         - Fixed passing AsClip() a NULL argument during TFM and TFMPP object creation if no clip
               was given for clip2.  This would cause assertion failure when compiled in debug mode.


    12/19/2004  v0.9.6

         - Fixed not invoking a cache between TFM and TFMPP when PP > 4
         + Some internal additions to allow TDecimate to tell the difference between c matches
               and deinterlaced frames
         + Added debug output to d2v checking... when debug=true and a d2v file is specified it will
               report the type of d2v detected, the detected field order from the d2v if order = -1,
               and report the errors if any are found


    11/30/2004  v0.9.4

         + significant speed up (30-50%) to modes 1, 2, and 4 with PP > 0, due to some missing logic
              the output frame would needlessly get checked twice for combing


    11/28/2004  v0.9.3.1

         - Fixed crashing when mode = 0 or mode = 3 and PP was greater than 0, the conditions
              for an array allocation were not adjusted as needed when the PP option was
              added in v0.9.1


    11/28/2004  v0.9.3

         + Added crc checking to input/output files.  Whenever an output file is
              created, TFM creates a crc32 value based off the first 15 frames in
              the current clip.  When the file is loaded via the "input" option
              the crc value from the file is checked against the current clips crc
              value.


    11/27/2004  v0.9.2

         - Fixed "slow" and "mChroma" parameters defaulting to false instead of true
         - Fixed display option not writing any part of a line if the total line
              length exceeded the width of the frame instead of writing what would fit
         - Changed default cthresh value to 10
         - Changed default PP value to 6 (motion-adaptive cubic interpolation)
         + Added d2v and ovrDefault options
         + Added IsCombedIVTC() conditional function
         + Added cubic deinterlacing method
         + Re-did input/output parameters.  Files created via the output option can
              no longer be read via the ovr option!  You must use the input parameter
              to read files created via the output parameter!
         + Output option no longer requires linear access


    11/21/2004  v0.9.1

         - Changed default mode value to 1
         - Changed default MI value to 128
         - Allow blockx and blocky sizes up to 2048
         - Reordered the parameter syntax slightly
         + Added exclusion band (y0/y1)
         + Added post-processing (PP parameter) and related stuff
             - Added clip2 and mthresh parameters
         + Added hinting in preparation for tdecimate


    11/11/2004  v0.9.0

         - initial release



H.)  TO DO LIST:


    - bugfixes as needed for the 1.0 line



contact:   forum.doom9.org  nick = tritical  or  email:  kes25c@mizzou.edu
