

                              TDecimate v1.0.1  -  HELP FILE  (02/19/2007)



CONTENTS OF FILE:


    A.) General Info
    B.) Basic Parameters
    C.) Advanced Parameters
    D.) File Input/Output Parameters
    E.) Debug/Display Parameters
    F.) Overrides Info
    G.) Change List
    H.) To Do List



A.)  GENERAL INFO:


     * Currently TDecimate only supports YV12 and YUY2 colorspaces!

      TDecimate is a decimaton filter intended to remove duplicates from a video
   stream.  It supports a couple types of operation which include M-in-N decimation
   and an arbitrary framerate decimation scheme that can support ratios not achievable
   with M-in-N. It also includes special handling for hybrid material such as
   blend decimation (for a single frame rate solution) or vfr via mkv using a timecodes
   file.


   syntax=>

       	TDecimate(int mode, int cycleR, int cycle, float rate, float dupThresh, float vidThresh,
                  float sceneThresh, int hybrid, int vidDetect, int conCycle, int conCycleTP,
                  String ovr, String output, String input, String tfmIn, String mkvOut, int nt,
                  int blockx, int blocky, bool debug, bool display, int vfrDec, bool batch,
                  bool tcfv1, bool se, bool chroma, bool exPP, int maxndl, bool m2PA,
                  bool denoise, bool noblend, bool ssd, int hint, PClip clip2, int sdlim, int opt)



B.)  BASIC PARAMETERS:


    mode -

        Sets the mode of operation.  Possible settings:


           Mode 0 =  Straight M-in-N decimation.  TDecimate will examine each set of N
                     frames and decimate the M most similar frames.  The values of M and
                     N are controlled via the cycleR and cycle parameters.  Blend decimation
                     of video (30p) is supported in the this mode (hybrid = 1), as well as
                     blending of 24p into 30p (hybrid = 3).


           Mode 1 =  Exactly like mode 0, except instead of decimating the M most similar
                     frames, frames are decimated from the longest remaining strings of
                     duplicates. The duplicate detection uses the dupThresh parameter.  This
                     mode is the correct type of decimation for anime and other sources where
                     frames are repeated 2, 3 or 4 times in a row, and also supports blend
                     decimation of video (30p) with hybrid = 1, as well as blending of 24p
                     into 30p (hybrid = 3).


           Mode 2 =  This mode uses a separate decimation algorithm that can achieve any
                     arbitrary framerate.  It is useful when you cannot achieve the desired
                     framerate with M-in-N decimation. The output framerate for this mode is
                     set using the "rate" parameter.  The maxndl parameter can be used to
                     tweak behavior on sources with uneven duplicate distribution. No hybrid
                     handling can be used in this mode!

                     This modes output will be slightly different if you run it with a metrics
                     input file (created on a previous pass in mode 4 for example) that lets
                     it analyze the entire video at the very beginning than if you run it
                     straight and let it analyze the video as it goes.  Generally the differences
                     will be small, but the 2 pass method (i.e. full analysis from an input file)
                     will generally produce a smoother result.  The m2PA parameter can be used
                     to force the one pass version of mode 2 to produce the same results as the
                     two pass version by reading ahead in the stream as much as is required
                     (the one pass version limits the read ahead to 100 frames max).


           Mode 3 =  This is a one-pass vfr for mkv with timecodes output mode.  Hybrid must be
                     set to 2 in this mode!  It uses M-in-N decimation and cycleR must be set
                     to 1!  The type of decimation that is used on film sections (most similar or
                     longest string) is controlled via the vfrDec setting.  For this mode to work
                     all access must be linear from start to finish... an error will be thrown
                     if non-linear access is detected.

                     Since vfw needs to know the # of frames before processing starts this
                     mode does not change the # of frames and simply pads the output as needed
                     with black frames.  The last actual frame will be recorded as a comment at
                     the end of the mkv timecodes file, and will be reported on the padded frames
                     as well once at least 300+ extra frames are returned.  If the se option is
                     set to true, then TDecimate will throw an error once the 306th extra frame
                     is reached, stopping processing and alerting the user.  If your gonna be
                     around when its done and not doing batch encoding this option can save you
                     some time.

                     The name and path of the mkv timecodes file to output is set using the
                     mkvOut parameter.


           Mode 4 =  Metrics output.  No decimation is done, but metrics are calculated allowing
                     for the output, display, or debug options to be enabled and outputting of
                     the metrics for later use.  (first pass for two pass mkv vfr using mode 5)


           Mode 5 =  This is similar to mode 3 (mkv vfr, and requires hybrid=2 and cycleR=1), but
                     as part of a two pass process.  It requires a complete input file (obtained
                     via the output parameter on a previous pass), and a complete tfmIn file (see
                     the batch option for a way around these requirements).  The advantages of this
                     mode over Mode 3 are that it does not require linear access (seeking is
                     supported), it uses the conCycleTP parameter instead of the conCycle parameter
                     which allows for values greater than 2, and it will have a correct frame count
                     with no padded frames.

                     As of version 0.9.11.8 of TDecimate, an input and tfmIn file are no longer
                     required for mode 5.  If an input file is not specified then a value of
                     ULLONG_MAX-1 (the maximum value tdecimate has) is assigned to all metrics.
                     Likewise, if a tfmIn file is not specified then all matches are assigned as 'c',
                     not combed, and not a d2v duplicate.


           Mode 6 =  This is for doing 120fps->vfr w/ timecode file.  It requires a complete metrics
                     input file generated via mode 4 on a previous pass.  It will decimate bit for bit
                     identical frames only.  All decimation will be into one of the following frame
                     rates:  119.880, 59.940, 39.960, 29.970, 23.976.

           Mode 7 =  This mode is similar to mode 2 in that it uses a decimation algorithm that can
                     achieve any arbitrary framerate. However, it operates quite differently
                     from mode 2.  It is useful for when you cannot achieve the desired framerate
                     with M-in-N decimation and cannot afford to go with two-passes in mode 2 (in which
                     case mode 7 will usually give better results if the duplicate distribution is
                     at least somewhat consistent).

                     The output framerate for this mode is set using the "rate" parameter.  It
                     also uses the "dupthresh" and "vidthresh" parameters... dupthresh sets a
                     threshold such that any frames with difference values under dupthresh are
                     considered duplicates, and vidthresh sets a threshold such that any frames
                     with difference values above vidthresh are considered non-duplicates.  Frames
                     with difference values inbetween dupthresh and vidthresh are classified as
                     similar unless they represent a descernable local minimum or maximum in the
                     difference values string.  By default dupthresh is set to 0.5 and vidthresh
                     is set to 4.0 (they use the usual 0 to 100 normalized scale).


	Default:  0  (int)


    cycleR -

        Sets the "M" for the M-in-N decimation modes.  In other words, setting this to 1
        means 1 frame in every cycle frames will be dropped.  This setting can be
        anything in the range 1 to (cycle-1).  It must be less than the value of the cycle
        setting!

           *NOTE:  all hybrid handling options only support cycleR = 1.  So if hybrid > 0
                   this value must be set to 1!

	Default:  1  (int)


    cycle -

        Sets the "N" for the M-in-N decimation modes.  In other words, setting this to 5
        means cycleR frames in every 5 frames will be dropped.  This setting can be
        anything in the range 2 to (number of frames in video).  It must also be greater
        than the cycleR setting.

	Default:  5  (int)


    rate -

        This sets the output frame rate when using mode = 2 or 7.  Frames will be dropped
        so that this frame rate is acheived while keeping audio/video sync as close as
        possible.  This must be less than the input frame rate.

        Default:  23.976  (float)


    hybrid -

        Controls how or if video sections (30p) should be dealt with.  Possible
        settings:

            0 - no handling
            1 - blend decimation of 30p sections into 24p and leave 24p untouched   (modes 0 and 1)
            2 - vfr via mkv w/ timecodes file output                                (modes 3 and 5)
            3 - blend conversion of 24p sections into 30p and leave 30p untouched   (modes 0 and 1)

          * The hybrid option is not used when mode = 2 or mode = 4, and hybrid > 0
            is only currently supported for cycleR = 1!

        Default:  0  (int)


    vfrDec -

        Sets the type of decimation to use for film sections when using modes 3 and 5.
        Possible settings:

             0 - drop most similar frame in cycle
             1 - decimate from longest string of duplicates

        Default:  1  (int)



C.)  ADVANCED PARAMETERS:


    dupThresh - 

        This sets the threshold for duplicate detection.  This setting is used in mode 1
        and also in modes 3 and 5 if vfrDec = 1.  If the difference metric for a frame is less
        than or equal to this value then it is declared a duplicate.  NOTE:  metrics will be
        slightly different between YV12 and YUY2 processing if chroma=true... the metrics have
        been normalized so they should match closely, but on average the YUY2 metrics tend to be
        slightly higher (5-10%) than the YV12 metrics for the same frame when chroma=true.
        When chroma=false YV12 and YUY2 metrics will be the same, however chroma=false metrics
        will be higher than chroma=true metrics so if you set chroma=false be sure to account
        for this.  This value is a % of maximum change for a block defined by the blockx and
        blocky values.... so 1.1 means 1.1% of maximal possible change.

        When in mode 7, dupThresh is used to set a threshold below which frames are considered
        to absolutely be duplicates.  Use display=true to see what the calculated metric values
        for the frames are and what the threshold values (translated into unnormalized values) are.

	Default:  1.1  (if chroma = true)  (float) -- modes 1, 3, 5
                  1.4  (if chroma = false)

                  0.4  (if chroma = true)  (float) -- mode 7
                  0.5  (if chroma = false)


    vidThresh -

        This setting is used for detecting video sections (30p) based off frame metrics
        when hybrid > 0.  If all frames in a cycle have metrics above this threshold then
        the cycle is declared video metrics wise.  This setting is similar to dupThresh,
        but should be set slightly higher if your vidDetect setting is set to 1 and not 3.
        If you know that your source has a lot of video sequences then set this lower vs if
        you know your source is pure film then you can set this really high to prevent any
        possible misdetections.  This value is a % of maximum change for a block defined by
        the blockx and blocky values.... so 1.1 means 1.1% of maximal possible change.

        When in mode 7, vidThresh is used to set a threshold above which frames are considered
        to absolutely be non-duplicates.  Use display=true to see the unnormalized threshold
        values and the frame difference values.

        Default:  1.1  (if chroma = true)  (float) -- modes 1, 3, 5 && hybrid > 0
                  1.4  (if chroma = false)

                  3.5  (if chroma = true)  (float) -- mode 7
                  4.0  (if chroma = false)


    sceneThresh -

        Sets the threshold for detecting scene changes when using blend decimation for video
        sections (hybrid = 1) or blend conversion for 24p->30p (hybrid = 3).  This value is a
        % of maximum change for the luma plane.  Good values are between 10 and 15.  Must be
        in the range 0 to 100.

        Default:  15  (float)


    vidDetect -

        This sets what is required for single cycle video detection when hybrid > 0. Whether
        a single cycle alone is enough or whether two consecutive cycles or more must be
        detected as video is controlled via the "conCycle" and "conCycleTP" parameters.

        Video detection via frame matches:   (Labeled Type A)

            i.)  The matches that were used by TFM do not indicate that there are duplicates
                     in the cycle

        Video detection via metrics:   (Labeled Type B)

            i.)  All frames in the cycle have metrics above vidThresh.

        Video detection via absence of local minima:  (Labeled Type C)

            i.)  All frames in the cycle have metrics that are within 150% of each other (1.5x)
                 and within 2.0 (abs value difference) of each other.  The maximum metric value
                 within the cycle must greater than or equal to 0.3.

        How these types of information are used as a whole to determine video sections
        is determined by vidDetect.  Each vidDetect setting has a condition that if met will
        result in the current cycle being detected as video.  (refer above for the A and B
        labels).  Please note that ovr (overrides) overrules vidDetect!

           0 - A        (if matches indicate video then consider it video)
	   1 - B        (if metrics indicate video then consider it video)
	   2 - A or B   (if either matches or metrics indicate video then consider it video)
	   3 - A and B  (if both matches and metrics indicate video then consider it video)
           4 - A and (B or C)  (if matches indicate video and metrics indicate video or
                                matches indicate video and there are no local minima consider
                                it video)

        Default:  3  (int)


    conCycle -

        conCycle sets the required minimum # of consecutive cycles detected as video for any
        section to be considered video when hybrid > 0.  Meaning, if conCycle is set to 2, and
        a single cycle is detected as video but both the cycle before it and after it are
        detected as film then that cycle will be considered film as well.  If conCycle had been
        set to 1 in the previous example then the standalone video cycle would have been consider
        video.  This setting is used in all cases except two pass mkv vfr (mode 5) where
        conCycleTP is used instead!  The difference is conCycle is limited to a maximum value of
        2 while conCycleTP has no upper limit.  Possible values are 1 or 2.

        default:  1  if vidDetect = 3  (int)
                  2  otherwise


    conCycleTP -

        This is the same as conCycle, but is used in mode 5 (two pass) and allows for any
        value (not just 1 or 2) and has no upper limit.

        Default:  1  if vidDetect = 3  (int)
                  2  otherwise


    nt -

        Sets the noise threshold used when calculating difference metrics.  If the abs()
        difference between two pixels is less than or equal to this value, then the
        difference is considered 0.  This can help lower the metrics of actual duplicate
        frames thus widening the difference between dups and non dups making it easier to
        set correct thresholds.  Avoid setting this value to high or very similar objects
        moving over one another will start to not be detected etc... Good values are in the
        range 1-2.  For clean video using a value of 0 seems to work best.

        Default:  0  (int)


    blockx -

        Sets the x-axis size of the blocks used for metric calculations.  Larger blocks
        give better noise suppression, but also give worse detection of small movements.
        Possible values are any power of 2 from 4 up to 2048 (4, 8, 16, 32, ... 2048).

        Default:  32  (int)


    blocky -

        Sets the y-axis size of the blocks used for metric calculations.  Larger blocks
        give better noise suppression, but also give worse detection of small movements.
        Possible values are any power of 2 from 4 up to 2048 (4, 8, 16, 32, ... 2048).

        Default:  32  (int)


    batch -

        This setting is intended to be used only with mode 5. Basically, it sets some
        arrays to fake values and disables a few checks allowing for an avisynth script
        with tdecimate(mode=5, ...) to be loaded when the tfmIn and input files do not
        have any entries.  This is useful and needed for setting up a two pass system
        in vdub's job control.  i.e. you make the first pass and second pass scripts, and
        then set up both to encode in vdub's job control.  NOTE:  if you set batch = true
        and the tfmIn and input files do not have entries for all frames then you will
        get borked output!

        As of v0.9.12.3, batch also disables crc checking when using an input file (this
        applies to all modes), and it will only set arrays to fake values if mode is set
        to 5.

            true - enables fake values and disables checks
            false - doesn't

        Default:  false  (bool)


    tcfv1 -

        Sets the type of timecode format to use for mkv timecode files when they are
        created in modes 3 and 5.  The two format types are those defined and used
        by mkvtoolnix.  verion 1 sets the framerate for frame ranges while version 2
        gives the timecode for each frame in milliseconds.  See the mkvtoolnix documentation
        for more info about the two formats.

            true - use version 1
            false - use version 2

        Default:  true  (bool)


    se -

        Only used when in mode 3.  It will cause TDecimate to throw an error once the 306th
        padded frame is reached, alerting the user that it has finished, so that time wont be
        spent processing unneeded frames.  This option should not be used when doing batch
        encoding or something similar, because the error will usually pop-up a window which requires
        the user to click, thus it would stop any subsequent processing as well.

            true - stop early (throw error)
            false - don't

        Default:  false (bool)


    chroma -

        Sets whether or not chroma is considered when calculating frame difference metrics.
        Setting this to false can give a speed up... it a quality vs speed setting (though
        in some cases setting chroma=false can improve operation).

            true - consider chroma
            false - don't

        Default:  true (bool)


    exPP -

        Set this to true if you're using a tfmIn file, have tfm set to PP=1, and are using a
        separate filter (such as tdeint) to do post-processing based on tfm's combed frame hints.
        If you don't set this to true when PP=1 in tfm, then tdecimate assumes the interlaced
        frames marked in the tfmIn file are not being deinterlaced... if this is not the case
        (they are actually being deinterlaced by a separate filter) then those frames will not
        be handled correctly.

        Default:  false (bool)


    maxndl -

        This setting is used only with mode 2 and stands for "max non-duplicate length".  It tells
        TDecimate the maximum consecutive number of non-duplicates. This info is used when planning
        the decimation strategy.  In normal cases, when duplicates are evenly distributed in the
        video, it should not be necessary to set this.  Only in cases where the length indicated
        by the decimation ratio is too short should this need setting.  For example, say we have
        the following pattern in a video:

                  5 5 7 7 2

        where the numbers indicate how many frames there are between duplicates.  In this case we
        want to remove 5 in every 26 frames.  This decimation ratio (5/26) would indicate that
        there is one duplicate in every 5.2 frames  (5/26 = 1/5.2).  Obviously, as the pattern
        above shows, this is the not the case as there are runs of up to 7 without a duplicate. So
        we would need to set maxndl to 7.

        Another example would be decimating a 59.94fps video to 23.976.  This ratio would indicate
        one duplicate in every 1.667 (5/3) frames.  However, if the video has sections where two
        non-duplicates are back to back then maxndl would need to be set to 2 to correctly handle it.


        EXTRA INFORMATION:

           While maxndl stands for "max non-duplicate length", it is actually more like a trade off
           between maintaining video sync and producing a smooth result.  The larger maxndl is the
           more the decimation can be non-uniformly spread throughout the video, which helps the 
           smoothness of the result in cases where duplicates are not evenly spread.  Anyways,
           experiment with increasing maxndl and see what happens.


        Possible settings for maxndl are any integer greater than 0.

        Default:  not set  (int)


    m2PA -

        Will override the default read-ahead maximum of 100 for mode 2.  This will allow the
        one pass mode (metrics not available from an input file) to produce the same results
        as if the metrics were available.

         **NOTE:  the cycle size could very well be in the 1000's or 10000's, so there is the
                  possibility setting m2PA=true could mean the processing will stall for quite
                  some time (5-10 minutes or more) when a new cycle starts!!!  Please check the
                  largest cycle size that will be used using debug=true before setting m2PA=true!

           true = override the default maximum
           false = don't

        Default:  false  (bool)


    noblend -

        Even with hybrid=0 there is a special case when tdecimate will use blend decimation, and
        that is when it detects two duplicates in a cycle, cycleR=1, and neither duplicate is next
        to a scenechange.  In such cases tdecimate will drop one of the duplicates and replace the
        other with a blend of its neighbors.  The "noblend" parameter is used to disable this so
        that no blending is ever done when hybrid = 0.

           true - no blending when hybrid = 0
           false - use blending in the two duplicate case

        Default:  true  (bool)


    denoise -

        Sets whether or not to denoise frames prior to doing difference metric calculations.
        This can greatly improve metrics for noisy sources (i.e. stabilize duplicate frame
        metrics and make it easier to tell the difference between duplicates and non-duplicates).
        It also works very well for sources with lots of dot-crawl because the denoising
        effectively cancels all dot-crawl, whereas the dot-crawl would usually inflate difference
        values of duplicates.  Using denoising will slow things down somewhat, but it is MMX
        optimized and pretty fast.

          true - use denoising
          false - don't

        Default:  false (bool)


     ssd -

        Controls whether the metrics are calculated as SAD (sum of absolute differences) or SSD
        (sum of squared differences).

           true - use ssd
           false - use sad

          ** Prior to v0.9.11.0 of tdecimate SAD was always used... and it is almost always best
             for TDecimate's purposes and the default thresholds for dupThresh, vidTresh, and
             sceneThresh are based on SAD values.

        Default:  false (bool)


     hint -

        Enables or disables reading of tfm's hints.  The information in the hints can effect
        tdecimate's decisions (i.e. in mode 0 it can lead to dropping a frame other than the
        lowest metric'd frame in a cycle).  Hint information contains match used, combed vs.
        progressive, d2v rff info... that info is also used for hybrid detection (depending
        on the vidDetect setting).  true enables reading, false disables.  If not explicitly
        set by the user, tdecimate checks if hints are present in the stream on load and sets
        the 'hint' parameter accordingly.

        Default:  auto-detect on load (bool)


     clip2 -

        Allows specification of a second clip from which to take frames. Metric calculation
        and decimation are still done on the input clip, but the frames that tdecimate
        returns are from clip2.  Clip2 must have the same number of frames are the input clip
        and be in YUY2 or YV12 colorspace (it does not have to have the same colorspace as
        the input clip).

        Default:  null (PClip)


     sdlim -

        When using mode 0, 1, or 3, with cycleR > 1, sdlim sets the minimum distance in frames
        between removed duplicates.  For example, with sdlim=2, tdecimate will not remove any
        frame that is within two frames of a frame already marked for decimation.  Frames are
        marked for decimation in order from lowest to highest difference metric within the current
        cycle.  The maximum value for sdlim is governed by the following equation:

                 (sdlim+1)*(cycleR-1) < cycle 

        When using longest string decimation (mode 1 or mode 3 w/ vfrdec=1), sdlim will only come
        into play if the number of frames with difference metrics < dupthresh is < cycleR-1.

        It is possible to use an sdlim value that could result in tdecimate not being able to
        mark a full cycleR worth of frames.  In this case, if sdlim is positive (i.e. > 0), then
        tdecimate will mark as many frames as possible with the given sdlim value and then simply
        mark the remaining number frames without regard to how close they are to already marked frames.
        If sdlim is negative (i.e. < 0), then tdecimate will decrease sdlim for that cycle by 1 and
        then start over from scratch marking frames.  This process of decreasing sdlim will continue
        until a value that allows a full cycleR worth of frames to be marked is found.  When sdlim
        is given as a negative value, the absolute value is actually used.  The sign is simply used
        to determine which method of dealing with the "unable to mark a full cycleR worth of frames"
        scenario is used.

        Default:  0  (int)


     opt -

         Controls which optimizations are used.  Possible settings:

            0 - use c routines
            1 - use mmx routines
            2 - use isse routines
            3 - use sse2 routines
            4 - auto detect

         Default:  4  (int)



D.)  FILE INPUT/OUTPUT PARAMETERS:


   ovr -

        Sets the name and path to an overrides file.  An overrides file can be used to
        force ranges of frames to be considered film or video and to specify drop frames
        or decimation patterns over ranges of frames.  For more info on using an ovr file
        see the OVERRIDES section at the bottom of this file.

        Default:  ""  (String)


   output -

        Sets the name and path to an output file.  The output file will include all metrics
        caculated.  Each line will include a frame number, plus the difference metric, and
        the scene change metric.  This file can be used for input (via the input parameter)
        on another pass to avoid having to recalculate the metrics or for the mode 5 two pass
        vfr support.

        Default:  ""  (String)


   input -

        Sets the name and path to a metrics file to use as input.  This file should have
        been created with the "output" parameter on a previous pass.

        Default:  ""  (String)


   tfmIn -

        Sets the name and path to an output file from TFM.  This option is useful when using
        hint=true and a tfm output file has been generated on a previous pass.  This option
        allows TDecimate to get info from tfm without having to check frames for hints, which
        can result in a very large speed up for large cycle sizes (even small cycle sizes should
        get a noticable speed increase). The only case where a tfmIn file is absolutely required
        is in mode 5!

        Default:  ""  (String)


   mkvOut -

        This sets the name and path for the mkv timecodes file that is generated in
        modes 3 and 5.

        Default:  ""  (String)



E.)  DEBUG/DISPLAY PARAMETERS:


     debug -

        Enabling this will make TDecimate output information about its internal states and
        decisions via OutputDebugString().  You can use a program called DebugView from
        System Internals:

                        http://www.sysinternals.com/ntw2k/utilities.shtml

        to view this output.  This can be useful in setting thresholds and seeing what is 
        happening.  To find out exactly what all it shows you'll have to use it ;)

        When mode = 2 and debug=true, TDecimate will spit out the cycle sizes for the
        series of M-in-N decimations.  That output will look something like this:

                     [1004] mode2_cfs 0 = 7
                     [1004] mode2_cfs 1 = 7
                     [1004] mode2_cfs 2 = 14
                     [1004] mode2_cfs 3 = 56
                     [1004] mode2_cfs 4 = 392

        The last "mode2_cfs # = ##" line shows the largest cycle size being used (the number
        after the "=").  So if you set m2PA=true, and the metrics are not available from an
        input file, TDecimate will be reading that ## frames (392 in the above case) ahead
        in the video stream, and will have to process those many frames at each cycle boundary!

        default:  false  (bool)


     display -

        Outputs almost exactly the same information as debug, but draws it on the actual frames
        in the upper left hand corner.  This is usually easier to read and use then the debug
        output.  To find out exactly what all it shows you'll have to use it ;)

        default:  false  (bool)



F.)  OVERRIDES:


        An overrides file can be used to manually set drop frames, declare video/film sections,
        or specify decimation patterns over ranges of frames.


           specifying video cycles:

              To specify a range of frames for TDecimate to consider video... first, enter the
              starting frame number, then put a comma (","), then enter the ending frame number,
              and finally put a "v" as the specifier.  This range is inclusive, meaning that the
              starting and ending frame numbers will be counted as video! Remember that video
              sections are only considered when hybrid > 0!

              example:     10,334 v


           specifying film cycles:

              Same as video but use "f" as the specifier.  Doing this will only make a difference
              when using hybrid > 0 and detecting video sections.  In all the other modes everything
              is considered film to begin with.

              example:     10,334 f


           specifying drop frames:

              To specify a drop frame enter the frame number you want to drop and put a "-" specifier.
              If you manually specify more than cycleR drop frames for one cycle then the ones that come
              first chronologically will be used.  If using mode 2, and not an M-in-N decimation mode,
              the same restriction applies, but instead of cycleR being the limiter it is an internally
              computed number.

              example:     226 -


           specifying a decimation pattern:

              Use the drop frame specifier along with keep frame specifiers (+) as place holders.

              example:     10,334 +-+++

              In this example every 2nd frame will be dropped starting at frame 10 and going to
              frame 334. 


           EXTRA NOTES:

              1.) If you specify overlapping entries then the entry that comes last in the ovr
                  file will be used.

              2.) All frame number entries correspond to the frame numbers in the input clip
                  (i.e. the input into TDecimate).  They do not correspond to the frame numbers after
                  decimation (this is the cause of a lot of headaches).

              3.) You can only give cycleR drop frames per cycle.  If you specify more than that,
                  then the first cycleR worth specified will be used.



G.)  CHANGE LIST:


    19/02/2007  v1.0.1

         - fixed reading in tfm output files created with PP=0
         - fixed a bug in destroying hints on frame output
         - fixed a bug in drop/keep frame overrides in the last
              cycle of a video if the cycle was not full length


    18/01/2007  v1.0

         - nothing


    07/12/2006  v0.9.12.7

         - sdlim changes


    26/11/2006  v0.9.12.6

         + added sdlim parameter
         - expanded file input line buffers from 80 bytes to 1024 bytes
         - small change to debug output format of match/d2v duplicate info lines


    04/11/2006  v0.9.12.5

         - switch setfps() with muldivfps() for modes 0, 1, and 5
         - use FloatToFPS() from assumefps/changefps/convertfps for modes 2 and 7


    22/10/2006  v0.9.12.4

         + auto detect hints on load if hint is not explicitly set to true or false by the user
         + restore hints passed through tfm when outputting frames
         - fixed batch option setting arrays to fake values even if mode was not set to 5
         - fixed unneeded requesting of frames under certain conditions due to some logic errors
         - a few caching changes/fixes


    10/03/2006  v0.9.12.3

         + Removed maximum limit on cycle value (upper limit is now the # of frames in the video)
         + batch option now disables input file crc checking (applies to all modes)
         + Minor changes to tfm match and d2v aided decimation routines
         + Display crc values in error msg when crcs don't match


    07/26/2006  v0.9.12.2

         + set fps to average value of the clip in mode 5 (so duration stays the same)
         + use 6 decimal places in v2 tc output


    04/09/2006  v0.9.12.1

         - fixed opt parameter not be respected in the blurring functions used
              when predenoise=true


    03/23/2006  v0.9.12.0

         + Added clip2 parameter
         + Added hint parameter
         + Modes 0/1 fully support seeking when complete input/tfmIn files
             are present (tfmIn file not required if hint=false)
         - fixed a few mmx/isse routines containing paddq sse2 instruction
         - replace frame copy with makewritable where possible
         - fixed not allowing tfmIn file with hybrid=0
         - changed noblend default to true


    01/24/2006  v0.9.11.9

         + added opt parameter
         - fixed sse2 routines using psrldq


    01/19/2006  v0.9.11.8

         - don't require input and tfmIn files for mode 5


    01/17/2006  v0.9.11.7

         - sse2 optimizations (only used on P4)


    12/20/2005  v0.9.11.6

         - Fixed slow down problems with internal caching


    12/19/2005  v0.9.11.5

         + internal caching for modes 0, 1, and 3
         + show cycleR value in display output
         - Fixed a problem with display output wrap around for the drop frame #'s listing
         - Fixed metric prebuffering computing metrics for the incorrect frames within
              a cycle after a seek to a random frame.  It was causing a minor slow down
              when seeking.
         - Fixed requesting frames an extra time in modes 0, 1, and 3 when no
              field matching hints from tfm were present in the stream.


    12/18/2005  v0.9.11.4

         + wrap display=true text to multiple columns and mark frames that will
             be dropped with "**"
         + round to microsecond accuracy for all v1/v2 timecode output files
         + slightly more efficient metric cycle calculation


    12/04/2005  v0.9.11.3

         - Fixed bug in metric pre-buffering that would cause TDecimate to always throw
              an error when processing the last 2 cycles of a clip (introduced in v0.9.11.2).


    12/03/2005  v0.9.11.2

         + speeded up some of the mmx functions that were added in the last release
         + modes 0, 1, and 3 now pre-compute metrics for the next needed cycle while
              delivering frames for the current cycle in order to evenly distribute
              cpu usage


    11/21/2005  v0.9.11.1

         + optimized c metric calculation routine (~2.5-3x faster)
         + removed width restrictions on isse yuy2 scenechange detection routine
         + added mmx yuy2 scenechange detection routine
         + removed all pitch and width restrictions on isse sad/ssd block metric calculation routines
         + added mmx sad routines
         + require mmx and not isse for the assembly ssd routines because they use only mmx instructions
         + removed width restrictions on mmx denoise routines
         - fixed possible divide by zero crash with vidDetect = 4


    11/01/2005  v0.9.11.0

         + Added ssd parameter
         + Added vidDetect = 4 mode
         + Converted all metric storage/calculation to __int64 to prevent possible overflow
              on large frames
         - Fixed mode 0/1 incorrect decimation of the last cycle of a clip when cycleR > 1
              and the number of frames wasn't a multiple of the cycle length


    10/07/2005  v0.9.10.1

         + Expanded mode 7 display/debug output
         - Fixed a bug in mode 7's frame decision code


    09/28/2005  v0.9.10.0

         + Added "noblend" parameter (disable 2 drop scenario blending when hybrid=0)
         + Added mode 7, an arbitrary framerate decimation mode (like mode 2), but based on
              some ideas from smartdecimate
         + Added denoising parameter, enables denoising of frames before calculating difference
              values (good for noisy sources or sources with lots of dot-crawl)


    09/11/2005  v0.9.9.7

         - Fixed crash when reading in tfmIn files that did not have +/- markings


    09/02/2005  v0.9.9.6

         - Fixed vfrDec=0 crash due to heap corruption


    08/27/2005  v0.9.9.5

         + Added fast isse routine for 50/50 blending case
         - Fixed a bug in hybrid=3 operation that caused it to handle certain scenechange
              situations incorrectly.


    08/15/2005  v0.9.9.4

         + mode=1 w/ d2v info and hybrid=3 decimation improvements


    08/14/2005  v0.9.9.3

         + Added hybrid=3 handling (blend convert 24p sections into 30p)
         + Added generalized isse metric calculation routine (yv12 blocksizes 16x16 or up
              and yuy2 blocksizes 8x8 or up now use isse when nt <= 0 instead of only the
              32x32 case)


    06/25/2005  v0.9.9.2

         + Added mode 6 (120fps -> vfr w/ timecodes file)


    05/24/2005  v0.9.9.1

         + Added iSSE optimizations for default metric calculation path 
              (32x32 blocks + nt<=0 + mod 16 width and height)


    05/18/2005  v0.9.9

         + First cut at new mode 2 operation.
         + Added maxndl/m2PA parameters, go with mode 2.


    04/19/2005  v0.9.8.3

         + Added exPP parameter, fixes handling of interlaced frames marked in tfmIn files when
              PP=1 in tfm and an external post-processor is used to deinterlace the combed frames.
         - Fixed crash caused by above circumstances


    03/13/2005  v0.9.8.2

         + Added missing logic to most similar decimation mode.  It can now correctly handle
             panning->static and static->panning areas like longest string.  It can also detect
             cycles that need two duplicates dropped.  Assuming match info is present.
         + Tweaked decimation decisions for both longest string/most similar.  These are the decisions
             that use the extra info such as match info and d2v rff info from tfm.
         + Added isse luma diff calculation routine for yuy2
         - Fixed a bug in the longest string decimation decision that utilized match info from tfm.


    03/10/2005  v0.9.8.1

         + Scene change metrics are calculated using only luma, regardless of the chroma option
         + There can only be one change above sceneThresh within the current cycle as well as the
             surrounding two cycles for it to be detected as a scene change (as long as cycle length
             is 10 or less)
         + D2V rff duplicate info is taken into account when deciding what frames to drop, instead 
             of only for hybrid detection
         + When hybrid > 0 and concycle or concycleTP is greater than 1, single cycles that are detected
             as video and that have a scene change detected in them are treated as video


    02/19/2005  v0.9.8

         + Most similar decimation mode now takes duplicate via match info into account
         + Match duplicate info and d2v duplicate info is shown with debug/display options
         + rff info from d2v option in tfm is now taken into account when doing hybrid detection
         + Increased the maximum possible cycle value to 300


    01/08/2005  v0.9.7.2

         - Fixed SetCacheHints being called incorrectly and always defaulting to CACHE_ALL
         - Small change to protect against overflow with 1.0 weight when blending frames


    01/04/2005  v0.9.7.1

         + Improved longest string decimation algo by having it look for an obvious duplicate case
               based off matches/metrics


    01/03/2005  v0.9.7

         - Fixed mode 4 display output saying "mode 3" instead of "mode 4"
         + Added chroma parameter
         + mode 4 display and debug output now display the sceneChange metrics along with the
               block difference metrics


    01/02/2005  v0.9.6.2

         - Fixed incorrect setcachehints call due to checking the value of the wrong argument
         + Faster and more accurate mmx/sse2 blending routines, thanks to Leak
         + Optimized the metric calculation routines.  Exactly how much of a speed increase is dependent
               on the source being processed.
         + Some other optimizations and internal changes.


    12/22/2004  v0.9.6.1

         - Fixed a problem with timecode file generation that would occur in mode 5 with tcfv1 = true.
               If the cycle following a cycle that needed 2 dups removed was detected as video then
               an erroneous line would be written to the file.
         - Fixed not initializing mkvOutF file handle


    12/19/2004  v0.9.6

         - Fixed not differentiating between c matches and deinterlaced frames when hybrid > 0
               and checking for dups via matches
         - Fixed crash with debug=true and large cycles (> 50) due to too small of a string buffer
         - Changed default sceneThresh to 13
         - conCycle and conCycleTP now default to 1 when vidDetect = 3 and still default to 2
               when vidDetect != 3
         + Added handling for cycles around scene changes which need 2 dups removed
         + Some other internal changes


    12/14/2004  v0.9.4

         - Fixed problems with longest string decimation and static to panning and panning to
               static scene workarounds in longest string decimation
         + added se parameter (causes mode 3 to stop early once the last actual frame is delivered)
         + mmx and sse2 blending routines now work with any width (not just mod 8 and mod 16)


    12/07/2004  v0.9.3

         - fixed outputting of extra timecode entries when using tcfv1=false (v2 format) in
               mode 3 or mode 5 and the last frame was not a cycle boundary
         - fixed incorrect formatting of the first 2 lines of the mkvOut file when
               in mode 3 and using tcfv1=false (v2 format)
         + added mmx and sse2 blending routines (used when hybrid = 1)


    11/30/2004  v0.9.2

         - fixed mishandling of the last cycle of a clip when in mode 3 and the
               last cycle was film
         - removed a mode 5 specific vidDetect = 3 action that wasn't suppose to be there
         + write blockx and blocky sizes into tdecimate metric log files
         + timecode v2 format support


    11/28/2004  v0.9.1

         + Added batch parameter
         + Added crc checking of input/output files to make sure that a file loaded via the
              input parameter actually goes with the current video


    11/27/2004  v0.9

         - Initial release



H.)  TO DO LIST:


    - bugfixes as needed for the 1.0 line



contact:   forum.doom9.org  nick = tritical  or  email:  kes25c@mizzou.edu
