Configuring router to run SDM |
Follow the instructions below to configure a router to run SDM. Step 1: Connect to your router using Telnet, SSH or via console. Enter the global configuration mode using the command: Router>enable Router#conf terminal Router(config)# Step 2 : Enable the router's HTTP/HTTPS server, using the following Cisco IOS commands: Router(config)# ip http server Router(config)# ip http secure-server Router(config)# ip http authentication local Note:- HTTPS is enabled only for crypto enabled IOS images. Step 3: Create a user with privilege level 15. Router(config)# username <username> privilege 15 password 0 <password> Note:- Replace <username> and <password> with the username and password that you want to configure. Step 4: Configure SSH and Telnet for local login and privilege level 15: Router(config)# line vty 0 4 Router(config-line)# privilege level 15 Router(config-line)# login local Router(config-line)# transport input telnet Router(config-line)# transport input telnet ssh Router(config-line)# exit Step 5: (Optional) Enable local logging to support the log monitoring function: Router(config)# logging buffered 51200 warning