;-------------------------------------------------------------------------
; jswpslwfx.inf -- JumpStart WPS Filter Driver 
;
; Copyright (c) Atheros.  All rights reserved.
;-------------------------------------------------------------------------
[version]
Signature   	= "$Windows NT$"
Class     	= NetService
ClassGUID  	= {4D36E974-E325-11CE-BFC1-08002BE10318}
Provider    	= %athr%
DriverVer	= 05/15/2008,1.0.0.50
Catalogfile     = jswpslwfx.cat

[Manufacturer]
%athr%=ATHR,NTx86,NTia64,NTamd64

[ATHR.NTx86]
%AthSec_Desc%=Install, MS_NdisLwf

[ATHR.NTia64]
%AthSec_Desc%=Install, MS_NdisLwf

[ATHR.NTamd64]
%AthSec_Desc%=Install, MS_NdisLwf

;-------------------------------------------------------------------------
; Installation Section
;-------------------------------------------------------------------------
[Install]
AddReg=Inst_Ndi
Characteristics=0x40000
NetCfgInstanceId="{ef19862d-07b9-4bc2-bca9-7dd7f64462e4}"
Copyfiles = AthSec.copyfiles.sys

[SourceDisksNames]
1=%AthSec_Desc%,"",,

[SourceDisksFiles]
jswpslwfx.sys=1

[DestinationDirs]
DefaultDestDir=12
AthSec.copyfiles.sys=12

[AthSec.copyfiles.sys]
jswpslwfx.sys,,,2


;-------------------------------------------------------------------------
; Ndi installation support
;-------------------------------------------------------------------------
[Inst_Ndi]
HKR, Ndi,Service,,"jswpslwf"
HKR, Ndi,CoServices,0x00010000,"jswpslwf"
HKR, Ndi,HelpText,,%AthSec_HelpText%
HKR, Ndi,FilterClass,, Custom
HKR, Ndi,FilterType,0x00010001,0x00000002
HKR, Ndi\Interfaces,UpperRange,,"noupper"
HKR, Ndi\Interfaces,LowerRange,,"nolower"
HKR, Ndi\Interfaces, FilterMediaTypes,,"ethernet"
HKR, Ndi,FilterRunType, 0x00010001, 1 ;this filter must run before any protocol can bind to the below miniport 

;-------------------------------------------------------------------------
; Service installation support
;-------------------------------------------------------------------------
[Install.Services]
AddService=JSWPSLWF,,AthSec_Service_Inst

[AthSec_Service_Inst]
DisplayName     = %AthSec_Desc%
ServiceType     = 1 ;SERVICE_KERNEL_DRIVER
StartType       = 1 ;SERVICE_SYSTEM_START
ErrorControl    = 1 ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\jswpslwfx.sys
LoadOrderGroup  = NDIS
Description     = %AthSec_Desc%
AddReg          = Common.Params.reg

[Install.Remove.Services]
DelService=JSWPSLWF,0x200

[Common.Params.reg]
; HKR, FilterDriverParams\DriverParam, 		ParamDesc, 	, "Jump Start parameter"
; HKR, FilterDriverParams\DriverParam, 		default, 	, "5"
; HKR, FilterDriverParams\DriverParam, 		type, 		, "int"

[Strings]
athr = "Atheros"
AthSec_Desc = "JumpStart Wireless Filter Driver"
AthSec_HelpText = "JumpStart Wireless Filter Device"





